Scintillator Test Update

Zelimir Djurcic, Matt Toups 21th August, 2007

Talking about:

-Apples to apples comparison of hole vs. groove and glue vs. no glue. -Future steps

The attenuation lengths were calculated to be 220.26cm for hole no glue (red), 164.2cm for hole with glue (blue), 200.9cm for groove no glue (pink), and 220.3cm for groove with glue (green).

We will:

-Finish measurements of 2m strip with the groove and no glue.

-Make measurements of 2m strip with the groove which we will glue.